Fusion of Tire Lateral Force Estimation and Sliding Mode Control for Torque Vectoring

Jinmin Kim1), Hyunseup Jo1) and Sang Won Yoon2)\*

1)Department of Automotive Engineering (Automotive – Computer Convergence), Hanyang University, Seoul 04763, Korea

2)Department of Electrical and Computer Engineering, Seoul National University, Seoul 08826, Korea

(Received date ; Revised date ; Accepted date ) \* Please leave blank

**ABSTRACT−**Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here.Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. Type the abstract here. [Capital letter at the beginning of each sentence, put a period at the end, Please write in 100 ~ 200 words, Times New Roman, 9pt]

**KEY WORDS** : Type key words here, Type key words here, Type key words here, Type key words here

nomenclature

*Vx* : longitudinal velocity, m/s

*Vy* : lateral velocity, m/s

γ : yaw rate, rad/s

*ax* : longitudinal acceleration, m/s2

*ay* : lateral acceleration, m/s2

*δ* : steering angle, rad

*Td* : wheel driving torque, N·m

*Tb* : wheel braking torque, N·m

|  |
| --- |
| subscripts  *FL, FR, RL, RR*: front left, front right, rear left, rear right |
| \* *Corresponding author*. e-mail: [swyoon@snu.ac.kr](mailto:swyoon@snu.ac.kr) |

*r* : effective radius of tire, m

*m* : vehicle mass, kg

*Iz* : moment of inertia about z axis, kg·m2

*lF* : distance from front axle to the center of gravity, m

*lR* : distance from rear axle to the center of gravity, m

*L* : wheel base length, m

*t* : half of track width, m

*h* : height from ground to the center of gravity, m

*Cα* : cornering stiffness, N/rad

*σ* : relaxation length, m

*μ* : road friction coefficient, -

1. INTRODUCTION

The manuscript elements have been formatted for you through the “styles” capability of the software. To use the styles, select the text you wish to apply a style to, then,

2. Estimation of Lateral tire force

In this section, we describe the lateral force estimation process using an Adaptive Extended Kalman Filter (AEKF) and introduce an offline optimization approach for modifying cornering stiffness. Lateral forces are influenced by various factors, including slip angle, road conditions, vertical load on the tire, and tire’s cornering stiffness. The estimation process consists of three main parts: (1) the vehicle lateral dynamics model under the three degrees of freedom (3-DoF), (2) vertical force calculation, and (3) a brief explanation of Dugoff’s tire model, which is widely used for its simplicity. However, Dugoff’s tire model assumes that cornering stiffness as a constant value, this can lead to inaccurate results in overall estimation as the slip angle increases.

To address this, an offline optimization approach is utilized to modify cornering stiffness, allowing it to more accurately represent the changing conditions as the slip angle increases. This is achieved through an axle distribution-based lateral force calculation method. The detailed full-wheel vehicle model is illustrated in Figure 1, and the equations of vehicle dynamics are formulated as follows (Doumiati *et al.*, 2011; Lee *et al*., 2018):

|  |  |
| --- | --- |
|  | (1) |
|  | (2) |
|  | (3) |

where  are the longitudinal velocity, lateral velocity, yaw rate, front left wheel steering angle, front right wheel steering angle, vehicle mass, moment of inertia about yaw axis, distance from front axle to the center of gravity (CG), distance from rear axle to the CG, half of track width and aerodynamic drag resistance, respectively. Tire forces,  and  (*i* denotes the axle position) represent the longitudinal and lateral forces with the subscript .



Figure 1. Representation of a four-wheel vehicle model

Lateral forces on the tire generated by the interaction with the road surface are primarily due to the presence of a slip angle. Therefore, calculating the slip angle is critical for determining lateral tire forces; this can be calculated as described in Eq. (4).

|  |  |
| --- | --- |
|  | (4) |

where  denotes the front left wheel steering angle and front right wheel steering angle.

2.1. Vertical tire force calculation

The vertical tire force plays a crucial role in accurately estimating lateral forces. It is essential to account for  through that consider load transfer and acceleration, as these are directly influenced during the vehicle’s dynamic behavior such as cornering, accelerating, and braking.

The couplings between pitch and roll dynamics are neglected in this study, assuming that these have a minimal effect on the overall vertical force calculation. The vertical forces can be simplified and calculated using the approach outlined in Eq. (5) (Doumiati *et al.*, 2011).

|  |  |
| --- | --- |
|  | (5) |

where are the vehicle mass, gravitational acceleration, distance from ground to CG, half of track width, wheelbase length, longitudinal acceleration and lateral acceleration, respectively.

2.2. Dugoff’s tire model

To represent tire forces, Dugoff’s tire model combines both lateral and longitudinal tire forces. It calculates these forces based on the slip ratio of longitudinal forces and the slip angle for lateral forces. By neglecting longitudinal slip ratio, simplified Dugoff’s tire model for lateral force is described in Eq. (6) (Dugoff *et al*., 1970).

|  |  |
| --- | --- |
|  | (6) |

where represent the cornering stiffness of each axle, and  is the tire-road friction coefficient, assumed to be 1.0 for a high-friction road surface. Meanwhile, the lateral force is generated with a time lag relative to change in slip angle, it causes transient response of the tire. The lateral tire force dynamics is first order and represented as follows (Guenther *et al*., 1990, Heydinger *et al*., 1991):

|  |  |
| --- | --- |
|  | (7) |

Here, denotes the relaxation length, which is assumed to be constant value of 0.1m in this study.

2.3 Axle distribution based-lateral force

As mentioned before, the Dugoff’s tire model assumes that the lateral tire force is proportional to slip angle. However, this assumption is valid within a limited small range of slip angle. As slip angle increases, the behavior of the tire becomes nonlinear and no longer increases



Figure 2. Overall system diagram

proportionally with the slip angle, instead, it approaches a saturation points where additional increases in slip angle yield diminishing in lateral force. Thus, predicting the lateral tire force using linear models becomes less accurate.

On the other hand, an alternative approach is proposed for estimating lateral tire force without relying on tire modeling and filtering methods (Li *et al*., 2019). Instead, they predict the lateral tire force directly by focusing on the distribution of vertical load across the tires relative to the total load on certain axle. The equations of the axle distribution based lateral force calculation is described in Eq. (7).

|  |  |
| --- | --- |
|  | (8) |
|  | (9) |

Here,represents the lateral tire force,  and  are the total lateral forces on the front and rear axles, respectively.

2.4. Optimization for modifying cornering stiffness

According to T. D. Gillespie, load transfer affects cornering stiffness, and this relationship can be presented by a second-order polynomial with respect to vertical force. Previous studies have also explored this relationship between cornering stiffness and vertical force (Doumiati *et al*., 2011; Jeong *et al*., 2022). The second-order polynomial equation is adjusted by adding a bias termin this study as described in Eq. (10), where represents the initial cornering stiffness when side slip angle is small. While the axle distribution-based method does not fully capture the nonlinear relationship between lateral force and slip angle, it remains effective for modifying the cornering stiffness and reflecting nonlinear changes as the slip angle increases.

|  |  |
| --- | --- |
|  | (10) |
|  | (11) |

To further refine cornering stiffness, an optimization problem is then formulated aimed at reflecting the effect of vertical load, as defined in Eq. (12). This involves minimizing the sum of squared error between Eq. (8) and Eq. (11).

|  |  |
| --- | --- |
|  | (11) |

The Levenberg Marquardt method is utilized for this optimization task and the optimal values for the coefficients and as -0.006 and 3.501, respectively.

2.5. Adaptive extended kalman filter

To estimate the lateral force in state-space model, the AEKF is employed to dynamically adjust the process noise (Akhlaghi *et al*., 2017). Unlike the process noise, which is adjusted dynamically to reflect changes in the system state transitions, the measurement noise is kept constant and remain relatively stable under normal operating conditions. The AEKF utilizes 8-dimensional state vector , 5-dimensional input control vector , and 5-dimenstional measurement vector  as follows:

|  |  |
| --- | --- |
|  | (13) |
|  | (14) |

 is excluded from the state vector and used as an input control vector calculated by Eq. (14). It is determined by using the wheel driving torque, wheel braking torque, and the effective radius of the tire denoted as,, respectively. The priori state  of AEKF is calculated by integrating over discrete time deviation  as described in Eq. (12) ~ (13).

|  |  |
| --- | --- |
|  | (14) |

|  |  |
| --- | --- |
|  | (13) |

The measurement model is described in Eq. (15) ~ (16).

|  |  |
| --- | --- |
|  | (15) |
|  | (16) |

where denotes the white gaussian measurement noise and is represented as a nonlinear function of 

The entire estimation process during discrete time deviationis formulated in Eq. (16).

|  |  |
| --- | --- |
|  | (16) |

Here, are the state covariance matrix, system noise covariance, and measurement noise covariance. are the Jacobian matrices of the nonlinear function of Compared to conventional EKF process, AEKF adaptively adjust the system noise covariance matrix , by balancing the weight  between the  and the innovation  term.

3. Torque-vectoring

3.1. Adaptive Sliding Mode Controller Design

In this study, to ensure robustness, a SMC approach is utilized to achieve the desired momentum. Depending on which order of the sliding surface being controlled, it referred to as First-Order Sliding Mode (FOSM) and Second Order Sliding Mode (SOSM). FOSM is simple to design and requires low computational power, but it can cause chattering problems. On the other hand, SOSM effectively mitigates chattering issues and is therefore commonly applied in TV systems (Liang *et al*., 2020). However, FS vehicles are constrained by limited computational resources. Additionally, FOSM, when combined with methods to reduce chattering, provides sufficient performance for TV (de Carvalho Pinheiro *et al*, 2023).

There are several techniques to reduce chattering, including adding a low pass filter, replacing the signum function with a saturation function, and using adaptive control gain. while adding low pass filter can reduce chattering, it negatively impacts to controller’s performance. In this paper, the signum function, and adaptive control gain are employed to mitigate chattering.

To establish SMC for torque vectoring, the sliding surface is designed for the vehicle’s yaw rate to track the desired yaw rate. it is expressed as follows:

|  |  |
| --- | --- |
|  | (17) |

The process of setting the control input involves following two steps. First, establish the equivalent control, which ensures  under the assumption of no disturbances and can be determined by imposing .

|  |  |
| --- | --- |
|  | (18) |

Derivation of yaw rate is defined in Eq. (3). This equation can be partitioned into two components: one is , which consist of , as described in the following:

|  |  |
| --- | --- |
|  | (19) |

And the other is , which consists of , as described in the following:

|  |  |
| --- | --- |
|  | (20) |

Using above equations, eq.(X) can be substituted as follows:

|  |  |
| --- | --- |
|  | (21) |

where  is added to represent disturbances. The term, which can be controlled using braking and acceleration, is treated as a control input.  is associated with lateral forces that are difficult to achieve. for getting equivalent control input, neglecting and , the equivalent control input defined Eq. (22) (Liang *et al*., 2020; de Carvalho Pinheiro *et al*., 2023; Zhang *et al*., 2020; Goggia et al., 2014).

|  |  |
| --- | --- |
|  | (22) |

Originally, signum function is incorporated into the control input as a switching term. However, to reduce the chattering phenomenon, the signum function can be replaced by a saturation function (Truong *et al*., 2013). Consequently, control input is defined as follows:

|  |  |
| --- | --- |
|  | (22) |

where is the control gain for sliding mode control. To ensure the sliding surface converges in finite time, Lyapunov functions are used. According to Eq. (23). control gain must be over the .

|  |  |
| --- | --- |
|  | (27) |

This paper employs an adaptively adjusted switching gain, which is modified based on the results of the AEKF and the sliding surface. The AEKF results utilized to set the reference value to account for the uncertainties. However, due to the continuous oscillations observed in the AEKF output, there is a risk of using AEKF directly. To address this, the AEKF results are used as indicators that identify intervals where uncertainty is located. The corresponding equation is as follows:

|  |  |
| --- | --- |
|  | (27) |

where is reference value that defines the intervals, is the estimation of using AEKF  is bias term for extra disturbances.

where a is reference value that defines the intervals, my\_ is the estimation of my using AEKF B is the bias term accounting for extra disturbances. the method of adjusting switching gain based on the states of sliding variable effectively addressed chattering phenomena near the sliding manifold (Back *et al*., 2016). To prevent setting the excessive switching gain, a weight that reflects the conditions of the sliding variable is applied to the switching gain. this weight is managed according to the following rules

1. If the sliding variable is smaller than in the previous step. It is assumed sliding gain is appropriate. The weight is not update
2. To prevent divergence, if the sliding variable reaches a predefined maximum value, the weight is not updated.
3. If the sliding variable is larger than in the previous step, it indicates the need for a higher gain, prompting an increase in the update step.
4. If the sliding variable is smaller than the threshold and its sign has changed compared to the previous step, it suggests system convergence. The weight is updated to smaller
5. If there is a change in E\_AKF, it is regarded as a change in the environment. To handle this condition, the weight of switching gain is reset to 1.

Following these rules, the weight update can express as follows:

|  |  |
| --- | --- |
|  | (27) |

where  is weight,  is tunable variable that determines the amount of change in each step.

3.2. Torque Distribution

In Section 3.1, the desired momentum is generated using FOSM. To achieve this momentum, the vehicle utilizes both steering and torque distribution. The ratio of torque distribution can be calculated by optimization-based control-allocation to achieve a specific purpose (De Novovellis *et al*., 2013) or by distributing it equally. While applying optimization-based control-allocation can enhance the vehicle’s performance, this paper distributes torque equally to avoid the additional computational resources. However, the force generated by drivetrain is constrained. Therefore, if the part of more power distribution exceeded its maximum power. It cannot maintain its speed. Due to this constraint, in that case, the excess value is redistributed to the other motor.

4. Experiment and Results

The overall process of lateral force estimation, offline cornering stiffness optimization, and torque-vectoring as illustrated in Figure 2, was tested using the CarMaker simulation environment. The tests were conducted on a Formula Student car model, equipped with virtual GNSS/IMU sensor that had Gaussian noise added to simulate real-world sensor inaccuracies, providing a more realistic evaluation of the proposed method’s performance. The specific vehicle specifications are detailed in Table 1. Three distinct scenarios were employed to assess its effectiveness in estimating lateral forces and toque vectoring. The three test scenarios include:

1. Sinus steer test: this is commonly used to assess the response of a vehicle to rapidly varying steering angles. The specific conditions involved driving the vehicle at a constant speed of 40km/h, with a sinusoidal steering input ranging from  to  over a 5-second period
2. Steady steer test: this test represents a steady-state cornering condition. The vehicle maintained a speed of 45km/h while driving on a circular track with a road curvature 45 meters.
3. Racetrack test: this test represents a steady-state cornering condition. The vehicle maintained a speed of 45km/h while driving on a circular track with a road curvature 45 meters.

Table 1. Vehicle’s specifications


|  |  |  |  |
| --- | --- | --- | --- |
| Name | Value | Name1 | Value |
| Mass[kg] | 226.26 | Stiffness of Front Spring [N/m] | 35000 |
| Length of Body [m] | 1.6 | Stiffness of Rear Spring [N/m] | 35000 |
| Distance C.G to Front[m] | 0.813 | Damping of Front [m/s] | 35000 |
| Distance C.G to Rear[m] | 0.787 | Damping of Rear [m/s] | 2500 |
| Moment of Inertia x [kgm2] | 53.624 | Moment of Inertia Motor [kgm2] | 0.01 |
| Moment of inertia y [kgm2] | 134.629 | Max Motor Torque [Nm | 30 |
| Moment of inertia z [kgm2] | 146.827 | Gear Ratio | 12.3 |

4.1 AEKF Results



The results of estimator lateral forces and  during in test scenarios are presented Figure 3 (sinus steer test), Figure 4 (steady steer test) and Figure 5 (racetrack test). The root mean square error (RMSE) results are detailed in Table 2. In both cases, the estimator shows compliant performance, confirming its effectiveness.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| RMSE | *Fy,FL*  (N) | *Fy,FR*  (N) | *Fy,RL*  (N) | *Fy,RR*  (N) | *My*  (Nm) |
| Sinus | 94.73 | 106.11 | 74.44 | 65.71 | 78.24 |
| Steady | 44.35 | 49.44 | 46.70 | 34.96 | 24.26 |
| Racetrack | 219.40 | 227.52 | 126.60 | 123.41 | 141.15 |

Table 2. Type the caption here. Type the caption here




(a) (b)




(c)


Figure 3. Estimation results for (a) front lateral force, (b) rear lateral force, and (c) *My* in sinus steer test.



(a)




(b)




(c)


Figure 4. Estimation results of (a) front lateral force, (b) rear lateral force, (c) *My* in steady steer test.




(a)



(b)



(c)



(d)

Figure 5. Estimation results of (b) front lateral force, (c) rear lateral force, (d) *My* in racetrack test.

4.2. Torque Vectoring Results

4.2.1 Tuning of the sliding mode controller variables

The tuning of the variable’s alpha, beta, and theta is as follows:

1. Alpha: This parameter must be set considering the error of the AEKF. In section 4.1, the AEKF’s error during racing track test does not exceed 500. Therefore, α is set to 500 to accommodate this maximum error.
2. Beta: The value of β should consider the disturbance torque Md​. To determine this, the CarMaker reference values of lateral force, and longitudinal force are used to calculate yaw moments My, and Mx. According to Eq. (3), the multiply by inertia moment and derivation of yaw moment comprise Mx, My. The differences between these values can be interpreted as Md. Figure 5 shows results of Md on the racing track, where Md does not exceed 100Nm. Thus, Β is set to 100
3. Theta: The time step for updating weight is set to 10ms. If theta is set too high, the changes in the weight would occur too rapidly. For stability, theta is conservatively set to 0.01 in this paper.




Figure 6. Results of Md in the racing track

5. CONCLUSION

Type the contents of the conclusion here. Type the contents of the conclusion here. Type the contents of the conclusion here. Type the contents of the conclusion here. Type the contents of the conclusion here. Type the contents of the conclusion here. Type the contents of the conclusion here. Type the contents of the conclusion here. Type the contents of the conclusion here. Type the contents of the conclusion here. Type the contents of the conclusion here.

**ACKNOWLEDGEMENT−**This work was supported by Institute of Information & communications Technology Planning & Evaluation (IITP) grant funded by the Korea government (MSIT) (No.2022-0-01053, Development of Network Load Balancing Techniques Based on Multiple Communication/Computing/Storage Resources)

REFERENCES

[x0] Doumiati, M., Victorino, A.C., Charara, A. and Lechner, D., 2010. Onboard real-time estimation of vehicle lateral tire–road forces and sideslip angle. *IEEE/ASME Transactions on Mechatronics*, *16*(4), pp.601-614.

[x0] Lee, E., Jung, H. and Choi, S., 2018. Tire lateral force estimation using Kalman filter. *International Journal of Automotive Technology*, *19*, pp.669-676.

[x0] Dugoff, H., Fancher, P.S. and Segel, L., 1970. An analysis of tire traction properties and their influence on vehicle dynamic performance. *SAE transactions*, pp.1219-1243.

[x0] Loeb, J.S., Guenther, D.A., Chen, H.H.F. and Ellis, J.R., 1990. Lateral stiffness, cornering stiffness and relaxation length of the pneumatic tire. *SAE transactions*, pp.147-155.

[x0] Heydinger, G.J., Garrott, W.R. and Chrstos, J.P., 1991. The importance of tire lag on simulated transient vehicle response. *SAE transactions*, pp.362-374.

[x0] Li, L., d’Andréa-Novel, B. and Thorel, S., 2019, October. New online estimation algorithm of lateral tire-road coefficients based on Inertial Navigation System. In *2019 IEEE Intelligent Transportation Systems Conference (ITSC)* (pp. 3859-3866). IEEE.

[x0] Jeong, D., Ko, G. and Choi, S.B., 2022. Estimation of sideslip angle and cornering stiffness of an articulated vehicle using a constrained lateral dynamics model. *Mechatronics*, *85*, p.102810.

[x0] Akhlaghi, S., Zhou, N. and Huang, Z., 2017, July. Adaptive adjustment of noise covariance in Kalman filter for dynamic state estimation. In *2017 IEEE power & energy society general meeting* (pp. 1-5). IEEE.

[x1] Liang, J., Zhao, J., Dong, Z., Wang, Y. and Ding, Z.(2020). Torque Vectoring and Rear-Wheel-Steering Control for Vehicle's Uncertain Slips on Soft and Slope Terrain Using Sliding Mode Algorithm. IEEE Transactions on Vehicular Technology 69, 4, 3805-3815.

[x2] de Carvalho Pinheiro, H., Carello, M., and Punta, E. (2023). Torque vectoring control strategies comparison for hybrid vehicles with two rear electric motors. Applied Sciences 13, 14, 8109.

[x3] Zhang, L., Ding, H., Shi, J., Huang, Y., Chen, H., Guo, K., and Li, Q. (2020). An adaptive backstepping sliding mode controller to improve vehicle maneuverability and stability via torque vectoring control. IEEE Transactions on Vehicular Technology, 69, 3, 2598-2612.

[x4] Goggia, T., Sorniotti, A., De Novellis, L., Ferrara, A., Gruber, P., Theunissen, J., Steenbeke, D., Knauder,B. and Zehetner, J. (2014). Integral sliding mode for the torque-vectoring control of fully electric vehicles: Theoretical design and experimental assessment. IEEE Transactions on Vehicular Technology, 64(5), 1701-1715.

[x5] Truong, D. T., Meywerk, M., and Tomaske, W. (2013). Torque vectoring for rear axle using Adaptive Sliding Mode Control. 2013 international conference on control, automation and information sciences (ICCAIS), pp. 328-333.

[x6] De Novellis, L., Sorniotti, A.,and Gruber, P. (2013). Wheel torque distribution criteria for electric vehicles with torque-vectoring differentials. IEEE transactions on vehicular technology, 63, 4, 1593-1602.

[x7] Baek, J., Jin, M., and Han, S. (2016). A new adaptive sliding-mode control scheme for application to robot manipulators. IEEE Transactions on industrial electronics, 63, 6, 3628-3637.

\* The Harvard System of references is to be used.

\* In the body of the text a paper is to be referred to by the author’s Last Name with the year of publication in parentheses.

Example :

-One author (Last Name, Year)

-Two authors (Last Name and Last Name, Year)

-More than three authors (Last Name *et al*., Year)

Example :

-One author : (Huh, 2000)

-Two authors : (Incropera and DeWitt, 1990)

-More than three authors : (Park *et al*., 2002)

\* References should be listed together at the end of the paper in alphabetical order by author’s Last Name.

-Type in all Author’s name and Paper title

-Type in reference of this paper in the text.

-Transactions of the Korean Society of Automotive Engineers : *Trans. Korean Society of Automotive*

*Engineers*

IJAT : *Int. J. Automotive Technology*

\* Citing a minimum of one citation from the International Journal of Automotive Technology (IJAT) is recommended.

**1. Journals**

All Author(s)(Type Last Name, then first and middle initials). (Year). Paper title(Capital letter at the beginning of sentence). *Journal Name(Italic)* **Volume number(bold)**, **Issue number(bold)**, pp.−pp.

Example :

Huh, H. (2000). Identification of autobody crashworthiness for space- framed vehicle models by finite element limit analysis. *Int. J. Automotive Technology* **1**, **1**, 101−112.

**2. Books**

All Author(s)(Type Last Name, then first and middle initials). (Year). *Book Title(Italic, Capital letter at the beginning of each keyword)*. Edition number. Publisher. The Location of Publisher(City).

Example :

Incropera, F. P. and DeWitt, D. P. (1990*). Fundamentals of Heat and Mass Transfer*. 3rd edn. John Wiley & Sons. New York.

**3. Website**

All Author(s) or Title (Access Year). Detailed Address.

Example :

PermaPure LLC (2006). http://www.permapure.com/

Presentations/Fuel%20Cell%20Humidification%20

presentation.ppt

**4. Reports and User Guide**

All Author/Organization or Title (Year). Title. Organization. Serial number.

Example :

Green, P. (1980). A Computer Simulation of Headlamp Variables and Drivers Sight Distances: Operating Instructions. HSRI Technical Report. UM-HSRI-80-44.

AVL (2006). BOOST Ver. 5.0 User Guide.